English

Firmware Upgrade Process:

1. Connect the power cable to the DX5 II and the power outlet.

2. Connect the device's USB interface to a PC/Mac via a usb cable.

3. Turn off the device with the power switch on the back. Press and hold the knob, then power on with the power switch. The screen will show the current software version.

4. A removable drive will show up in the explorer on PC/Mac. Open the drive.

5. Extract the downloaded compressed file, then copy the .Topping file to the root directory of the drive. The drive will then eject itself and reconnect

6. Reopen the drive. A new file will be showing the current firmware version as "Update successful(Version.Vx.xx)" of which the "XX" is the new firmware version that indicates the firmware is successfully upgraded.

7. Turn off and on the device again. The upgrade is complete.

*****************************************************************************************

简体中文


固件升级步骤：

1. 将电源线连接DX5 II和电源插座。

2. 用一根USB数据线将DX5 II的USB接口和电脑USB接口相连。

3. 按住旋钮的同时，将后面板上的 电源开关 从关切换到开的状态，设备屏幕显示当前的软件版本。

4. 电脑上会出现一个“TOPPING FW”U盘，打开它。

5 将下载下来的压缩包解压，然后将压缩包内的.Topping固件文件复制到U盘，然后等待。。。（U盘会自动消失，然后重新识别）

6. 重新识别后，再次打开U盘，显示 “Update successful(Version.Vx.xx)“ 表示升级成功。

7. 设备断电，重新上电，升级完成。




